**USER ACCEPTANCE TEST PLAN**

|  |  |  |
| --- | --- | --- |
| Location |  |  |
| Time |  |  |
| Test Method |  |  |
| Tools |  |  |
| # Person in Charge | Seller |  |
|  | Buyer |  |

**TEST ITEM**

|  |  |  |
| --- | --- | --- |
| Test Item 1 |  | Package Completeness |
| Test Item 2 |  | General Specification |
| Test Item 3 |  | Network Function |
| Test Item 4 |  | Call Function |

Test Item 1 : Package Completeness

|  |  |  |  |
| --- | --- | --- | --- |
| **PACKAGE COMPLETENESS** | **REQUIREMENTS** | **TEST SCENARIO** | **RESULTS** |
| Phone | 1 unit | Physical Look |  |
| Battery | 1 unit | Physical Look |  |
| Charger | 1 unit | Physical Look |  |
| Data Cable | 1 unit | Physical Look |  |
| Headset | 1 unit | Physical Look |  |
| Compass | 1 unit | Physical Look |  |
| User Manual | 1 unit | Physical Look |  |
| Warranty Card | 1 unit | Physical Look |  |

Test Item 2 : General Specification

|  |  |  |  |
| --- | --- | --- | --- |
| **GENERAL SPECIFICATION** | **REQUIREMENTS** | **TEST SCENARIO** | **RESULTS** |
| Model | Bar | Physical Look |  |
| Display | 1.5” | Physical Look |  |
| Colour | 65 K | Physical Look |  |
| Battery | Li-Ion | Physical Look |  |

Test Item 3 : Network Function

|  |  |  |  |
| --- | --- | --- | --- |
| **NETWORK FUNCTION** | **REQUIREMENTS** | **TEST SCENARIO** | **RESULTS** |
| Dual Band GSM Frequency | GSM 900/1800Mhz | Put 900/1800 MHz SIM Card and activate single mode option |  |
| Data | GPRS | Activate GPRS |  |
| Registration Applet | Support prepaid registration applet | Insert new prepaid SIM card |  |

Test Item 4 : Call Function

|  |  |  |  |
| --- | --- | --- | --- |
| **CALL FUNCTION** | **REQUIREMENTS** | **TEST SCENARIO** | **RESULTS** |
| Receiving call | Communication established by answering the call | Call using other phone |  |
| Making outgoing call | Communication established by originating the call | Call other phone using |  |
| Call Waiting | Call waiting text displayed in screen | Call using other phone while is in communication with other phone |  |
| Hold a call | Communication still established after answering other phone | Call using other phone while is in communication with other phone and answering call |  |
| Swap between calls | Communication still established after answering other phone and vice versa | Switch the call while in communication |  |
| Make new call during an on-going call | Communication still established after make new call | Call other phone using while in communication |  |
| USSD transactions including existing USSD applications such as reload, check balance, USSD Menu browser. | Receive USSD information after originate application code | Input code based on applications selected |  |